From c155562ad7a8f3808df9c4bf3c463bdc8a08c9a0 Mon Sep 17 00:00:00 2001
From: Luka Perkov <luka@openwrt.org>
Date: Fri, 12 Oct 2012 12:13:56 +0000
Subject: update switch documentation

SVN-Revision: 33733
---
 docs/network.tex | 23 ++++++++++++++++++++++-
 1 file changed, 22 insertions(+), 1 deletion(-)

(limited to 'docs/network.tex')

diff --git a/docs/network.tex b/docs/network.tex
index 5516bd9a30..cf1200dcd4 100644
--- a/docs/network.tex
+++ b/docs/network.tex
@@ -107,7 +107,7 @@ The name for the route section is optional, the \texttt{interface}, \texttt{targ
 \texttt{gateway} options are mandatory.
 Leaving out the \texttt{netmask} option will turn the route into a host route.
 
-\subsubsection{Setting up the switch (currently broadcom only)}
+\subsubsection{Setting up the switch (broadcom only)}
 
 The switch configuration is set by adding a \texttt{'switch'} config section.
 Example:
@@ -152,6 +152,27 @@ Three interfaces will be automatically created using this switch layout :
 You can then assign those interfaces to a custom network configuration name
 like \texttt{lan}, \texttt{wan} or \texttt{dmz} for instance.
 
+\subsubsection{Setting up the switch (swconfig)}
+
+\emph{swconfig} based configurations have a different structure with one extra
+section per vlan. The example below shows a typical configuration:
+
+\begin{Verbatim}
+config 'switch' 'eth0'
+        option 'reset' '1'
+        option 'enable_vlan' '1'
+
+config 'switch_vlan' 'eth0_1'
+        option 'device' 'eth0'
+        option 'vlan' '1'
+        option 'ports' '0 1 2 3 5t'
+
+config 'switch_vlan' 'eth0_2'
+        option 'device' 'eth0'
+        option 'vlan' '2'
+        option 'ports' '4 5t'
+\end{Verbatim}
+
 \subsubsection{Setting up IPv6 connectivity}
 
 OpenWrt supports IPv6 connectivity using PPP, Tunnel brokers or static
-- 
cgit v1.2.3

