From b9a7b48297bd3fcbaf56ffe948c1ff6c4825a697 Mon Sep 17 00:00:00 2001
From: Jo-Philipp Wich <jow@openwrt.org>
Date: Tue, 22 Sep 2009 16:17:05 +0000
Subject: [package] [docs] implement doth (802.11h) and wmm (802.11e) options
 for broadcom as well; update docs

git-svn-id: svn://svn.openwrt.org/openwrt/trunk@17676 3c298f89-4303-0410-b956-a3cf2f4a3e73
---
 docs/wireless.tex | 10 ++++++++++
 1 file changed, 10 insertions(+)

(limited to 'docs/wireless.tex')

diff --git a/docs/wireless.tex b/docs/wireless.tex
index d92fa76cd9..16dcd689fe 100644
--- a/docs/wireless.tex
+++ b/docs/wireless.tex
@@ -121,6 +121,8 @@ config wifi-iface
     option port     port
     option hidden   0,1
     option isolate  0,1	(broadcom)
+    option doth     0,1	(atheros, broadcom)
+    option wmm      0,1	(atheros, broadcom)
 \end{Verbatim}
 
 \paragraph{Options for the \texttt{wifi-device}:}
@@ -230,6 +232,14 @@ config wifi-iface
         Optional: Isolation is a mode usually set on hotspots that limits the clients to communicate only with the AP and not with other wireless clients.
         0 disables ap isolation (default); 1 enables ap isolation.
 
+    \item \texttt{doth} \\
+        Optional: Toggle 802.11h mode.
+        0 disables 802.11h (default); 1 enables it.
+
+    \item \texttt{wmm} \\
+        Optional: Toggle 802.11e mode.
+        0 disables 802.11e (default); 1 enables it.
+
 \end{itemize}
 
 \paragraph{Mesh Point}
-- 
cgit v1.2.3

