From 91f7c80407af6080d4f4fa08054c3d74730671a4 Mon Sep 17 00:00:00 2001
From: Andy Boyett <agb@openwrt.org>
Date: Sat, 31 Jan 2009 16:15:18 +0000
Subject: wireless.tex: update docs to reflect txpower move

SVN-Revision: 14311
---
 docs/wireless.tex | 8 ++++++--
 1 file changed, 6 insertions(+), 2 deletions(-)

(limited to 'docs/wireless.tex')

diff --git a/docs/wireless.tex b/docs/wireless.tex
index bc41b0e054..dd6ec43dd9 100644
--- a/docs/wireless.tex
+++ b/docs/wireless.tex
@@ -102,12 +102,13 @@ config wifi-device    wifi device name
     option hwmode     11b, 11g, 11a, 11bg (atheros, mac80211)
     option rxantenna  0,1,2 (atheros, broadcom)
     option txantenna  0,1,2 (atheros, broadcom)
+    option txpower  transmission power in dBm
 
 config wifi-iface
     option network  the interface you want wifi to bridge with
     option device   wifi0, wifi1, wifi2, wifiN
     option mode     ap, sta, adhoc, monitor, or wds
-    option txpower  transmission power in dBm
+    option txpower  (deprecated) transmission power in dBm
     option ssid     ssid name
     option bssid    bssid address
     option encryption none, wep, psk, psk2, wpa, wpa2
@@ -152,6 +153,9 @@ config wifi-iface
     \item \texttt{txantenna} \\
 	Optional: Antenna identifier (0, 1 or 2) for emission. This feature is supported by atheros and some broadcom chipsets.
 
+    \item \texttt{txpower}
+	Set the transmission power to be used. The amount is specified in dBm.
+
 \end{itemize}
 
 \paragraph{Options for the \texttt{wifi-iface}:}
@@ -192,7 +196,7 @@ config wifi-iface
 	Set the BSSID address to be used for wds to set the mac address of the other wds unit.
 
     \item \texttt{txpower}
-	Set the transmission power to be used. The amount is specified in dBm.
+	(Deprecated, set in wifi-device) Set the transmission power to be used. The amount is specified in dBm.
 
     \item \texttt{encryption} \\
         Encryption setting. Accepts the following values:
-- 
cgit v1.2.3

