From 096a28394e2f8f1399a07ef47e47fb5a5106ed26 Mon Sep 17 00:00:00 2001
From: Florian Fainelli <florian@openwrt.org>
Date: Wed, 1 Aug 2007 08:47:40 +0000
Subject: Fix a typo in the agmode selection

SVN-Revision: 8296
---
 docs/wireless.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'docs/wireless.tex')

diff --git a/docs/wireless.tex b/docs/wireless.tex
index 7a7d528e8c..67be1d2aa0 100644
--- a/docs/wireless.tex
+++ b/docs/wireless.tex
@@ -25,7 +25,7 @@ config wifi-iface
 config wifi-device      "wifi0"
     option type         "atheros"
     option channel      "5"
-    option mode  	"11g"
+    option agmode  	"11g"
 
 config wifi-iface
     option device       "wifi0"
@@ -77,7 +77,7 @@ config wifi-device     wifi device name
     option channel  1-14
     option maxassoc 1-128 (broadcom only)
     option distance 1-n
-    option mode     11b, 11g, 11a, 11bg (atheros only)
+    option agmode     11b, 11g, 11a, 11bg (atheros only)
 
 config wifi-iface
     option network  the interface you want wifi to bridge with 
-- 
cgit v1.2.3

